Frame 108 (227 bytes on wire, 227 bytes captured)
Ethernet II, Src: 00:03:47:31:51:a5, Dst: 00:50:ba:38:cd:b2
Internet Protocol Version 6
Transmission Control Protocol, Src Port: 36464 (36464), Dst Port: 554 (554), Seq: 3349886915, Ack: 3200203478, Len: 141
Real Time Streaming Protocol
    DESCRIBE rtsp://geryon.ctie.monash.edu.au/test_qcif_200_aac_64.mp4 RTSP/1.0\r\n
    CSeq: 1\r\n
    Accept: application/sdp\r\n
    User-Agent: Cisco RTSP 1.0\r\n
    \r\n

Frame 111 (1386 bytes on wire, 1386 bytes captured)
Ethernet II, Src: 00:50:ba:38:cd:b2, Dst: 00:03:47:31:51:a5
Internet Protocol Version 6
Transmission Control Protocol, Src Port: 554 (554), Dst Port: 36464 (36464), Seq: 3200203478, Ack: 3349887056, Len: 1300
Real Time Streaming Protocol
    RTSP/1.0 200 OK\r\n
    Server: DSS/4.0 [v410]-Linux\r\n
    Cseq: 1\r\n
    Last-Modified: Thu, 01 May 2003 23:08:35 GMT\r\n
    Cache-Control: must-revalidate\r\n
    Content-length: 1206\r\n
    Date: Thu, 04 Sep 2003 03:03:19 GMT\r\n
    Expires: Thu, 04 Sep 2003 03:03:19 GMT\r\n
    Content-Type: application/sdp\r\n
    x-Accept-Retransmit: our-retransmit\r\n
    Content-Base: rtsp://geryon.ctie.monash.edu.au/test_qcif_200_aac_64.mp4/\r\n
    \r\n
Session Description Protocol
    Session Description Protocol Version (v): 0
    Owner/Creator, Session Id (o): StreamingServer 3271633399 1051830515000 IN IP6 3ffe:8001:12:fc::4
    Session Name (s): /test_qcif_200_aac_64.mp4
    URI of Description (u): http:///
    E-mail Address (e): admin@
    Connection Information (c): IN IP4 0.0.0.0
    Time Description, active time (t): 0 0
    Session Attribute (a): control:*
    Session Attribute (a): isma-compliance:1,1.0,1
    Session Attribute (a): mpeg4-iod: "data:application/mpeg4-iod;base64,AoCAgwMAT///DwH/A4CAgggAB0DkZGF0YTphcHBsaWNhdGlvbi9tcGVnNC1vZC1hdTtiYXNlNjQsQVlDQWdRa0JnSUNBTVFLZkE0Q0FnQ29BQlFBRWdJQ0FGRUFWQUFFa0FBR0M0QUFCZUgwRmdJQ0FBaElRQm9DQWdBa0JBQU
    Session Attribute (a): range:npt=0-  22.83973
    Media Description, name and address (m): video 0 RTP/AVP 96
    Media Attribute (a): rtpmap:96 MP4V-ES/90000
    Media Attribute (a): control:trackID=2
    Media Attribute (a): mpeg4-esid:1
    Media Attribute (a): fmtp:96 profile-level-id=1; config=000001b0

Frame 113 (369 bytes on wire, 369 bytes captured)
Ethernet II, Src: 00:50:ba:38:cd:b2, Dst: 00:03:47:31:51:a5
Internet Protocol Version 6
Transmission Control Protocol, Src Port: 554 (554), Dst Port: 36464 (36464), Seq: 3200204778, Ack: 3349887056, Len: 283
Real Time Streaming Protocol
    Data (283 bytes)

Frame 116 (259 bytes on wire, 259 bytes captured)
Ethernet II, Src: 00:03:47:31:51:a5, Dst: 00:50:ba:38:cd:b2
Internet Protocol Version 6
Transmission Control Protocol, Src Port: 36464 (36464), Dst Port: 554 (554), Seq: 3349887056, Ack: 3200205061, Len: 173
Real Time Streaming Protocol
    SETUP rtsp://geryon.ctie.monash.edu.au/test_qcif_200_aac_64.mp4/trackID=2 RTSP/1.0\r\n
    CSeq: 2\r\n
    Transport: RTP/AVP;unicast;client_port=1024-1025\r\n
    User-Agent: Cisco RTSP 1.0\r\n
    \r\n

Frame 118 (441 bytes on wire, 441 bytes captured)
Ethernet II, Src: 00:50:ba:38:cd:b2, Dst: 00:03:47:31:51:a5
Internet Protocol Version 6
Transmission Control Protocol, Src Port: 554 (554), Dst Port: 36464 (36464), Seq: 3200205061, Ack: 3349887229, Len: 355
Real Time Streaming Protocol
    RTSP/1.0 200 OK\r\n
    Server: DSS/4.0 [v410]-Linux\r\n
    Cseq: 2\r\n
    Last-Modified: Thu, 01 May 2003 23:08:35 GMT\r\n
    Cache-Control: must-revalidate\r\n
    Session: 8130203433559886669\r\n
    Date: Thu, 04 Sep 2003 03:03:19 GMT\r\n
    Expires: Thu, 04 Sep 2003 03:03:19 GMT\r\n
    Transport: RTP/AVP;unicast;client_port=1024-1025;source=3ffe:8001:12:fc::4;server_port=6970-6971;ssrc=1659C617\r\n
    \r\n

Frame 121 (251 bytes on wire, 251 bytes captured)
Ethernet II, Src: 00:03:47:31:51:a5, Dst: 00:50:ba:38:cd:b2
Internet Protocol Version 6
Transmission Control Protocol, Src Port: 36464 (36464), Dst Port: 554 (554), Seq: 3349887229, Ack: 3200205416, Len: 165
Real Time Streaming Protocol
    PLAY rtsp://geryon.ctie.monash.edu.au/test_qcif_200_aac_64.mp4/ RTSP/1.0\r\n
    CSeq: 3\r\n
    Range: npt=0-22.8397\r\n
    Session: 8130203433559886669\r\n
    User-Agent: Cisco RTSP 1.0\r\n
    \r\n

Frame 123 (227 bytes on wire, 227 bytes captured)
Ethernet II, Src: 00:50:ba:38:cd:b2, Dst: 00:03:47:31:51:a5
Internet Protocol Version 6
Transmission Control Protocol, Src Port: 554 (554), Dst Port: 36464 (36464), Seq: 3200205416, Ack: 3349887394, Len: 141
Real Time Streaming Protocol
    RTSP/1.0 200 OK\r\n
    Server: DSS/4.0 [v410]-Linux\r\n
    Cseq: 3\r\n
    Session: 8130203433559886669\r\n
    RTP-Info: url=trackID=2;seq=32983;rtptime=928906259\r\n
    \r\n

Frame 140 (105 bytes on wire, 105 bytes captured)
Ethernet II, Src: 00:50:ba:38:cd:b2, Dst: 00:03:47:31:51:a5
Internet Protocol Version 6
User Datagram Protocol, Src Port: 6970 (6970), Dst Port: 1024 (1024)
Real-Time Transport Protocol
    Version: RFC 1889 Version (2)
    Padding: False
    Extension: False
    Contributing source identifiers count: 0
    Marker: True
    Payload type: Unknown (96)
    Sequence number: 32983
    Timestamp: 928906259
    Synchronization Source identifier: 374982167
    Payload: 000001B003000001B509000001000000...

Frame 141 (146 bytes on wire, 146 bytes captured)
Ethernet II, Src: 00:50:ba:38:cd:b2, Dst: 00:03:47:31:51:a5
Internet Protocol Version 6
User Datagram Protocol, Src Port: 6971 (6971), Dst Port: 1025 (1025)
Real-time Transport Control Protocol
Real-time Transport Control Protocol
Real-time Transport Control Protocol

Frame 142 (1510 bytes on wire, 1510 bytes captured)
Ethernet II, Src: 00:50:ba:38:cd:b2, Dst: 00:03:47:31:51:a5
Internet Protocol Version 6
Fragmentation Header
User Datagram Protocol, Src Port: 6970 (6970), Dst Port: 1024 (1024)
Real-Time Transport Protocol
    Version: RFC 1889 Version (2)
    Padding: False
    Extension: False
    Contributing source identifiers count: 0
    Marker: False
    Payload type: Unknown (96)
    Sequence number: 32984
    Timestamp: 928906259
    Synchronization Source identifier: 374982167
    Payload: 000001B610001843B110783FF5414E0C...